

**Selected Dimensions**

|  |
| --- |
| Bucket |
| G. Dump Clearance at Max Raise | 10.1 ft in | 3070 mm |
| Dimensions |
| A. Length with Bucket on Ground | 26.3 ft in | 8020 mm |
| B. Width Over Tires | 9.3 ft in | 2845 mm |
| C. Height to Top of Cab | 11.1 ft in | 3375 mm |
| D. Wheelbase | 10.5 ft in | 3200 mm |
| E. Ground Clearance | 1.5 ft in | 450 mm |
| F. Hinge Pin - Max Height | 13.4 ft in | 4090 mm |
| H. Reach at Max Lift and Dump | 3.7 ft in | 1120 mm |

**Specification**

|  |
| --- |
| Engine |
| Make | Komatsu |
| Model | SA6D108E |
| Displacement | 436.3 cu in | 7.2 L |
| Number of Cylinders | 6 |
| Operational |
| Operating Weight | 42218.5 lb | 19150 kg |
| Fuel Capacity | 75.8 gal | 287 L |
| Turning Radius | 22.1 ft in | 6730 mm |
| Transmission |
| Number of Forward Gears | 4 |
| Number of Reverse Gears | 4 |
| Max Speed - Forward | 18 mph | 28.9 km/h |
| Max Speed - Reverse | 18.1 mph | 29.1 km/h |
| Bucket |
| Dump Clearance at Max Raise | 10.1 ft in | 3070 mm |
| Bucket Width | 9.6 ft in | 2925 mm |
| Dimensions |
| Length with Bucket on Ground | 26.3 ft in | 8020 mm |
| Width Over Tires | 9.3 ft in | 2845 mm |
| Height to Top of Cab | 11.1 ft in | 3375 mm |
| Ground Clearance | 1.5 ft in | 450 mm |
| Wheelbase | 10.5 ft in | 3200 mm |
| Hinge Pin - Max Height | 13.4 ft in | 4090 mm |
| Reach at Max Lift and Dump | 3.7 ft in | 1120 mm |

New & Used Heavy Equipment <http://www.ritchiespecs.com/specification?type=Constructi&category=Wheel+Loader&make=Komatsu&model=WF350-3&modelid=91668#ixzz4vm1gU3MW>