
**Komatsu D65S-6 Crawler Loader**



**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Dimensions | | |
| A. Length with Bucket on Ground | 19 ft in | 5790 mm |
| B. Width to Outside of Tracks | 7.7 ft in | 2355 mm |
| C. Height to Top of Cab | 9.8 ft in | 2990 mm |
| G. Clearance at Full Height and Dump | 9 ft in | 2730 mm |
| H. Reach at Dump Height | 4.3 ft in | 1300 mm |
| Undercarriage | | |
| I. Track Gauge | 74 in | 1880 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Make | Cummins | |
| Model | NH220-CI | |
| Net Power | 160 hp | 119.3 kw |
| Displacement | 743 cu in | 12.2 L |
| Operational | | |
| Operating Weight | 39683.2 lb | 18000 kg |
| Fuel Capacity | 74 gal | 280 L |
| Cooling System Fluid Capacity | 14.5 gal | 55 L |
| Static Tipping Load | 11300 lb | 5125.6 kg |
| Breakout Force - Std Bucket | 14020 lb | 62.4 kN |
| Bucket Capacity - heaped | 2.4 yd3 | 1.8 m3 |
| Max Speed | 6.1 mph | 9.8 km/h |
| Undercarriage | | |
| Track Shoe Width | 18.1 in | 460 mm |
| Number of Track Rollers per Side | 6 | |
| Length of Track on Ground | 8.6 ft in | 2635 mm |
| Ground Pressure | 10.5 psi | 72.6 kPa |
| Track Gauge | 74 in | 1880 mm |
| Dimensions | | |
| Length with Bucket on Ground | 19 ft in | 5790 mm |
| Width to Outside of Tracks | 7.7 ft in | 2355 mm |
| Height to Top of Cab | 9.8 ft in | 2990 mm |
| Clearance at Full Height and Dump | 9 ft in | 2730 mm |
| Reach at Dump Height | 4.3 ft in | 1300 mm |