|  |  |
| --- | --- |
| **Technical specifications:** | **L6.5** |
| Production year model/type | 2000-2005 |
| Engine: | Perkins |
| Cil/Turbo/intercooler**:** | 4 |
| Engine model: | 704-30 |
| Capacity in Kw/Hp/Rpm: | 42/56,7/2300 |
| Maximum torque: Nm/rpm: | 210/1600 |
| Displacement (cm³) | 3000 |
| Fuel: | Diesel |
| Transmission: | 3 speed Hydrostatic |
| **Hydrauliek system:** |  |
| Capacity hydraulic tank (liter) | 60 |
| Capacity hydraulic system (liter) | x |
| Pump flow capacity: (ltr/min) | 62 |
| Maximum working pressure: (bar) | 210 |
| **Dimensions with bucket:** |  |
| Operating weight with st. bucket: (kg) | 4850 |
| Overal lenght with st. bucket (mm) | 5340 |
| Width over tires (mm) | 1925 |
| Machine width with st. bucket (mm) | 2050 |
| Height to top of cab (mm) | 2755 |
| Tires: | 365/80 R20 |
| Wheelbase lenght: (mm) | 2250 |
| Minimum turning Circle over bucket: (mm) | x |
| Bucket capacity struck (M³) | 0,7 |
| Bucket capacity heaped (M³) | 0,9 |
| Fuel tank (liter) | 100 |
| **Performances:** |  |
| Bucket pin height at maximum lift: (mm) | 3145 |
| Normal loading capacity  (± kg) | 1950 |
| Static Tipping load straight (± kg) | x |
| Static Tipping load at full turn (± kg) | 3250 |
| Travel speed low/high (km/h) | 7,0-35 |