|  |  |
| --- | --- |
| Technical specifications: | L564 2 + 2 |
| Production year model/type | 1998-2005 |
| Engine: | Liebherr |
| Cil/Turbo/intercooler: | 6TI |
| Engine model: | D926 TI-E A2 |
| Capacity in Kw/HP/Rpm: | 183/249/2000 |
| Maximum torque: Nm/rpm: | 1074/1200 |
| Displacement (cm³) | 9960 |
| Fuel: | Diesel |
| Transmission: | Stepless Hydrostatic |
| Hydrauliek system: |  |
| Capacity hydraulic tank (liter) | 160 |
| Capacity hydraulic system (liter) | 240 |
| Pump flow capacity: (ltr/min) | 290 |
| Maximum working pressure: (bar) | 325 |
| Dimensions with bucket: |  |
| Operating weight with st. bucket: (kg) | 22480 |
| Overal lenght with st. bucket (mm) | 8730 |
| Width over tires (mm) | 2930 |
| Machine width with st. bucket (mm) | 3000 |
| Height to top of cab (mm) | 3540 |
| Tires: | 26.5 R25 |
| Wheelbase lenght: (mm) | 3450 |
| Minimum turning Radius over bucket: (mm) | 6990 |
| Bucket capacity struck (M³) | x |
| Bucket capacity heaped (M³) | 4 |
| Fuel tank (liter) | 330 |
| Performances: |  |
| Bucket pin height at maximum lift: (mm) | 4355 |
| Normal loading capacity  (± kg) | 8850 |
| Static Tipping load straight (± kg) | 16800 |
| Static Tipping load at full turn (± kg) | 14750 |
| Travel speed low/high (km/h) | 10,0-40,0 |