

**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Dimensions | | |
| A. Length with Bucket | 12.5 ft in | 3833 mm |
| B. Width Over Tires | 5.5 ft in | 1676 mm |
| C. Height to Top of Cab | 6.8 ft in | 2083 mm |
| D. Wheelbase | 4.5 ft in | 1381 mm |
| E. Ground Clearance | 8.8 in | 225 mm |
| F. Length w/o Bucket | 10.7 ft in | 3265 mm |
| G. Clearance at Max Lift and Dump | 8.2 ft in | 2487 mm |
| H. Reach at Max Lift and Dump | 30 in | 764 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Make | Caterpillar | |
| Model | 3044C DIT | |
| Gross Power | 94 hp | 70 kw |
| Net Power | 90 hp | 67 kw |
| Power Measured @ | 2500 rpm | |
| Displacement | 201 cu in | 3.3 L |
| Number of Cylinders | 4 | |
| Operational | | |
| Operational Weight | 8292 lb | 3761 kg |
| Fuel Capacity | 26 gal | 98 L |
| Cooling System Fluid Capacity | 3.7 gal | 14 L |
| Engine Oil Fluid Capacity | 2.6 gal | 10 L |
| Hydraulic System Fluid Capacity | 15 gal | 57 L |
| Chain Box Fluid Capacity - each side | 2.9 gal | 11 L |
| Max Speed | 7.2 mph | 11.6 km/h |
| Operating Voltage | 12 V | |
| Alternator Supplied Amperage | 90 amps | |
| Loader | | |
| Operating Load Rating | 3250 lb | 1474 kg |
| Tipping Load | 6500 lb | 2948 kg |
| Breakout Force | 7315 lb | 3318 kg |
| Bucket Capacity | 0.52 yd3 | 0.4 m3 |
| Hydraulic | | |
| Pump Flow Capacity | 22 gal/min | 84 L/min |
| Relief Valve Pressure | 3335 psi | 23000 kPa |
| Dimensions | | |
| Length with Bucket | 12.5 ft in | 3833 mm |
| Length w/o Bucket | 10.7 ft in | 3265 mm |
| Width Over Tires | 5.5 ft in | 1676 mm |
| Height to Top of Cab | 6.8 ft in | 2083 mm |
| Clearance at Max Lift and Dump | 8.2 ft in | 2487 mm |
| Wheelbase | 4.5 ft in | 1381 mm |
| Ground Clearance | 8.8 in | 225 mm |
| Reach at Max Lift and Dump | 30 in | 764 mm |
| Turning Radius from Center - machine rear | 58.3 in | 1481 mm |
| Turning Radius from Center - inc bucket | 101.5 in | 2577 mm |

New & Used Heavy Equipment <http://ritchiespecs.com/specification?category=Skid%20Steer%20Loader&make=CATERPILLAR&model=272c&modelid=92084#ixzz4wFJLkC9l>