**Caterpillar D9G гусеничный гидравлический бульдозер с отвалом 9R Rip**

**** Представленный в 1961 году в качестве замены Cat D 9 E, d9g был самым крупным бульдозером, произведенным на момент его внедрения. Благодаря широкому ассортименту инструментов и навесного оборудования D9G стал одним из самых мощных, производительных и универсальных станков в линейке Caterpillar®. Некоторые из наиболее заметных применений D9G были для толкания скреперов, хотя он может быть оснащен рыхлителями, одним из нескольких типов лопат, доступных, или сконфигурирован как DD9G с двумя тракторами D9 в тандеме для использования в самых разнообразных приложениях, где полная мощность двух тракторов была необходима.

Оснащен уникальным 9R Rip лезвием, эта машина идеально подходит для дробления твердого грунта, резки корней и удаление пней, рыхление вдоль высокой стены, и бульдозерами. Гидравлические клыки на каждом угле лезвия можно углубить до 12".

|  |  |
| --- | --- |
| **Model history** | |
| **Model introduced** | [**1961**](http://tractors.wikia.com/wiki/1961) |
| **Model discontinued** | [**1974**](http://tractors.wikia.com/wiki/1974) |
| **Model status** | **Discontinued** |
| **Preceded by** | [**Caterpillar D9E**](http://tractors.wikia.com/wiki/Caterpillar_D9G) |
| **Superseded by** | [**Caterpillar D9H**](http://tractors.wikia.com/wiki/Caterpillar_D9G) |
| **Engine Specification** | |
| **Engine make** | **Caterpillar** |
| **Engine model** | **D353** |
| **Fuel type** | **Diesel** |
| **Power hp** | **385** |
| **Power kW** | **287** |
| **No. of Cylinders** | **6** |
| **Cooling system** | **Water** |