
**CATERPILLAR d8k Crawler Tractor**



**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Dimensions | | |
| A. Length w/ Blade | 21.6 ft in | 6580 mm |
| B. Width Over Tracks | 9.2 ft in | 2790 mm |
| C. Height to Top of Cab | 11.2 ft in | 3400 mm |
| D. Length of Track on Ground | 10.3 ft in | 3150 mm |
| E. Ground Clearance | 1.4 ft in | 434 mm |
| F. Length w/o Blade | 17.3 ft in | 5260 mm |
| Undercarriage | | |
| G. Track Gauge | 7 ft in | 2130 mm |
| H. Standard Shoe Size | 22 in | 559 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Model | D342 | |
| Gross Power | 300 hp | 223.7 kw |
| Displacement | 1244.9 cu in | 20.4 L |
| Operational | | |
| Operating Weight | 70503.8 lb | 31980 kg |
| Fuel Capacity | 169.1 gal | 640 L |
| Transmission | | |
| Type | powershift | |
| Number of Forward Gears | 3 | |
| Number of Reverse Gears | 3 | |
| Max Speed - Forward | 6.8 mph | 10.9 km/h |
| Max Speed - Reverse | 8.4 mph | 13.5 km/h |
| Undercarriage | | |
| Ground Pressure | 12.8 psi | 88.3 kPa |
| Ground Contact Area | 5456 in2 | 3.5 m2 |
| Standard Shoe Size | 22 in | 559 mm |
| Number of Track Rollers per Side | 5 | |
| Track Gauge | 7 ft in | 2130 mm |
| Standard Blade | | |
| Width | 13.3 ft in | 4040 mm |
| Dimensions | | |
| Length w/o Blade | 17.3 ft in | 5260 mm |
| Length w/ Blade | 21.6 ft in | 6580 mm |
| Width Over Tracks | 9.2 ft in | 2790 mm |
| Height to Top of Cab | 11.2 ft in | 3400 mm |
| Length of Track on Ground | 10.3 ft in | 3150 mm |
| Ground Clearance | 1.4 ft in | 434 mm |

# Caterpillar D8K бульдозер

Caterpillar D8K Гусеничный бульдозер с 3-х зубым рыхлителем.

спецификации Caterpillar D8K бульдозер

Двигатель Модель D342

Полная мощность 300 л.с. 223,7 кВт Объем 20,4 л

Эксплуатационная масса 70503,8 кг

Топливный бак 640 л

передачи вперед 3, назад 3

Максимальная скорость - Вперед 10,9 км / ч

Максимальная скорость - назад 13,5 км / ч

Шасси

Давление на грунт 88,3 кПа

Площадь опорной поверхности 3,5 м2

Стандартный размер 22 559 мм

Число опорных катков на сторону 5

Ширина колеи 2130 мм

Стандартный отвал

Ширина 4040 мм

Длина без лезвия 5260 мм

Длина ж / лезвия 6580 мм

Ширина За Треки 2790 мм

Высота до верха кабины 3400 мм

Длина гусеничной ленты 3150 мм

Дорожный просвет 434 мм

Высота до верха кабины 3400 мм

Длина гусеничной ленты 3150 мм

Дорожный просвет 434 мм