**International Harvester TD-24**

|  |  |
| --- | --- |
| Manufacturer | International Harvester |
| Model | TD-24 |
| Production | 1947 - 1959 |
| Standard engine | International Harvester  |
| MAX power | 83 kW / 113 hp (M) |
| MAX speed | 12 kmh / 7.5 mph |

|  |
| --- |
| GENERAL |
| Manufacturer | International Harvester |
| Fuel | Diesel |
| CONFIGURATION |
| POWER |
| Power Max | 125 kW / 170 hp (M) @ rpm |
| Power Drawbar Rated | 83 kW / 113 hp (M) |
| Power Drawbar Tested | 125 kW / 170 hp (M) |
| DIMENSIONS |
| Displacement | 17871 ccm / 17.9 L / 1090 cin |
| Cylinders | 6 |
| Bore | 146.00 mm / 5.748 inch |
| Stroke | 178.00 mm / 7.008 inch |
| compression | 15.22:1 |
| COOLING |
| Cooling | Water-cooling |
| Coolant | 140 L / 37 gal |
| OIL AND FUEL |
| Fuel capacity | 322 L / 85 gal |
| OTHER DATA |
| Rated RPM | 1375 rpm |
| GENERAL |
| Weight | 17599 kg / 38799 lb |
| Length | 463 cm / 182.3 inch |
| Width | 259.1 cm / 102 inch |
| Height | 242.1 cm / 95.3 inch |
| GENERAL |
| Weight | 17599 kg / 38799 lb |
| Chasis | selection\_data.chasis\_C |
| Batteries number | 4 |
| Battery voltage | 6 V |
| GENERAL |
| Short name | 8/8 |
| Full name | 8/8 |
| Type | Manual |
| GEARS |
| Gears Forward | 8 |
| Gears Reverse | 8 |
| Powershifts Forward | 0 |
| Powershifts Reverse | 0 |
| Reverser |
| SPEEDS |
| MAX Speed | 12 kmh / 7.5 mph |
| MIN Speed | 2 kmh / 1.2 mph |