
**Caterpillar D10 Crawler Tractor**



**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Dimensions | | |
| A. Length w/ Blade | 24.8 ft in | 7566 mm |
| B. Width Over Tracks | 12 ft in | 3647 mm |
| C. Height to Top of Cab | 14.9 ft in | 4535 mm |
| D. Length of Track on Ground | 12.8 ft in | 3911 mm |
| E. Ground Clearance | 2.3 ft in | 701 mm |
| F. Length w/o Blade | 19.4 ft in | 5915 mm |
| Undercarriage | | |
| G. Track Gauge | 9.5 ft in | 2896 mm |
| H. Standard Shoe Size | 28 in | 711 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Model | D348 | |
| Gross Power | 700 hp | 522 kw |
| Displacement | 1788 cu in | 29.3 L |
| Operational | | |
| Operating Weight | 171674 lb | 77870 kg |
| Fuel Capacity | 382 gal | 1446 L |
| Transmission | | |
| Type | powershift | |
| Number of Forward Gears | 3 | |
| Number of Reverse Gears | 3 | |
| Max Speed - Forward | 7.2 mph | 11.6 km/h |
| Max Speed - Reverse | 8.6 mph | 13.8 km/h |
| Undercarriage | | |
| Ground Pressure | 19.9 psi | 137.2 kPa |
| Ground Contact Area | 8618 in2 | 5.6 m2 |
| Standard Shoe Size | 28 in | 711 mm |
| Number of Track Rollers per Side | 8 | |
| Track Gauge | 9.5 ft in | 2896 mm |
| Standard Blade | | |
| Width | 11.4 ft in | 3480 mm |
| Dimensions | | |
| Length w/o Blade | 19.4 ft in | 5915 mm |
| Length w/ Blade | 24.8 ft in | 7566 mm |
| Width Over Tracks | 12 ft in | 3647 mm |
| Height to Top of Cab | 14.9 ft in | 4535 mm |
| Length of Track on Ground | 12.8 ft in | 3911 mm |
| Ground Clearance | 2.3 ft in | 701 mm |