**CATERPILLAR pr450 Cold Planer**

 

**Selected Dimensions**

|  |
| --- |
| Conveyor System |
| H. Discharge Conveyor Width | 30 in | 762 mm |
| Dimensions |
| A. Operating Length | 43.6 ft in | 13280 mm |
| B. Shipping Width | 9.4 ft in | 2870 mm |
| C. Shipping Height | 14 ft in | 4267 mm |

**Specification**

|  |
| --- |
| Engine |
| Make | Caterpillar |
| Model | 3408 |
| Gross Power | 450.6 hp | 336 kw |
| Displacement | 1098.4 cu in | 18 L |
| Operational |
| Operating Weight - Full Load | 56791.1 lb | 25760 kg |
| Fuel Capacity | 200 gal | 757.1 L |
| Water Spray System Fluid Capacity | 700 gal | 2649.8 L |
| Operating Speed | 175.9 ft/min | 53.6 m/min |
| Travel Speed | 2 mph | 3.2 km/h |
| Rotary Cutter |
| Cutting Width | 6.3 ft in | 1905 mm |
| Cutting Depth | 10 in | 254 mm |
| Number of Tools | 144 |
| Conveyor System |
| Discharge Conveyor Width | 30 in | 762 mm |
| Tracks |
| Number of Track Units | 3 |
| Front Track Width | 12 in | 305 mm |
| Rear Track Width | 12 in | 305 mm |
| Dimensions |
| Operating Length | 43.6 ft in | 13280 mm |
| Shipping Width | 9.4 ft in | 2870 mm |
| Shipping Height | 14 ft in | 4267 mm |