|  |
| --- |
| **Sumitomo HA60W-8** |
| **Paving Width** | **Standard (Min∼Max width)** | m | 2.3∼6.0 |
| **Pavingperformance** | **Paving thickness** | mm | 10∼300 |
| **Paving speed** | m/min | 1∼20 |
| **Hopper capacity** | ton | 13 |
| **Center crown ratio** | % | -1∼3 (slope 0∼3) |
| **Dimensions** | **Operating weight** | kg | 14,950 (L), 15,220 (E) \* |
| **Overall length** | mm | 6,930 |
| **Overall width** | mm | 2,490 |
| **Overall height (with canopy)** | mm | 2,765 (3,790) |
| **Transportation height (with canopy)** | mm | 2,765 (2,999) |
| **Wheel base / Tumbler distance** | mm | 2,700 |
| **Tiers** |   | Front 22 × 14 × 16 (solid) Rear 15.5R25 |
| **Conveyor system** | **Type of driving method** |  | Hydraulic (individual left & right) |
| **Width × No. of line** | mm | 482 × 2 |
| **Rotating speed** | m/min | 0∼15.9 |
| **Augersystem** | **Auger dimensions** | mm | 330 dia. × 300 pitch |
| **Rotating speed** | min-1 | 0∼82 |
| **Screed system** | **Model** |   | J.Paver 2360 |
| **Strike-off** | mm | Main screed: 81, Extension screed: 81 |
| **Heating system** |   | LPG blower burner / Electric (option) |
| **Compaction system** | **Type** |   | Tamper and vibrator / Vibrator (option) |
| **Vibrator frequency** | Hz | 0∼50 |
| **Tamper rotating speed** | Hz | 0∼20 |
| **Height adjustment of extendable screed** |   | Hydrostatic |
| **Height adjustment of extendable mold board** |   | Hydraulic |
| **Drive system** | **Type** |   | Wheel (Tier) |
| **Drive motor** |   | Front; Hyd. Motor / Rear; HST |
| **Brake type** |   | Automatic brake |
| **Traveling speed(Forward / Backward)** | km/h | 0∼15 / 0∼8 |
| **Engine** | **Make&Model** |   | ISUZU 4JJ1X |
| **Displacement** | cc | 2,999 |
| **Rated output** | kW/min-1 | 89.2 / 2,200 |
| **Fuel tank capacity** | L | 140 |
| **Electric system** | V | 24 |