

**Selected Dimensions**

|  |
| --- |
| Boom/Stick Option (HEX) 1 |
| A. Shipping Length of Unit | 36.4 ft in | 11100 mm |
| C. Shipping Height of Unit | 12.1 ft in | 3700 mm |
| I. Max Cutting Height | 28.5 ft in | 8686.8 mm |
| J. Max Loading Height | 21 ft in | 6400.8 mm |
| K. Max Reach Along Ground | 27.5 ft in | 8382 mm |
| L. Max Vertical Wall Digging Depth | 9 ft in | 2743.2 mm |
| M. Max Digging Depth | 12.8 ft in | 3901.4 mm |
| Dimensions |
| D. Length of Track on Ground | 11 ft in | 3368 mm |
| E. Ground Clearance | 1.5 ft in | 472 mm |
| G. Height to Top of Cab | 10.7 ft in | 3250 mm |
| H. Tail Swing Radius | 8.9 ft in | 2725 mm |
| O. Counterweight Clearance | 3.8 ft in | 1145 mm |
| Undercarriage |
| N. Shoe Size | 19.7 in | 500 mm |

**Specification**

|  |
| --- |
| Engine |
| Make | Liebherr |
| Model | D 924 T-E |
| Net Power | 132.8 hp | 99 kw |
| Power Measured @ | 2000 rpm |
| Aspiration | In-line engine water-cooled |
| Number of Cylinders | 4 |
| Operational |
| Operating Weight | 57320.2 lb | 26000 kg |
| Fuel Capacity | 95.1 gal | 360 L |
| Hydrauilc System Fluid Capacity | 60.8 gal | 230 L |
| Operating Voltage | 24 V |
| Alternator Supplied Amperage | 55 amps |
| Hydraulic System Relief Valve Pressure | 5221.4 psi | 36000 kPa |
| Hydraulic Pump Flow Capacity | 105.7 gal/min | 400 L/min |
| Undercarriage |
| Shoe Size | 19.7 in | 500 mm |
| Max Travel Speed | 3.1 mph | 5 km/h |
| Drawbar Pull | 60923.2 lb | 271 kN |
| Boom/Stick Option (HEX) 1 |
| Boom/Stick Option (HEX) 1 | 45degree attachment |
| Shipping Height of Unit | 12.1 ft in | 3700 mm |
| Shipping Length of Unit | 36.4 ft in | 11100 mm |
| Max Digging Depth | 12.8 ft in | 3901.4 mm |
| Max Reach Along Ground | 27.5 ft in | 8382 mm |
| Max Cutting Height | 28.5 ft in | 8686.8 mm |
| Max Loading Height | 21 ft in | 6400.8 mm |
| Max Vertical Wall Digging Depth | 9 ft in | 2743.2 mm |
| Dimensions |
| Height to Top of Cab | 10.7 ft in | 3250 mm |
| Ground Clearance | 1.5 ft in | 472 mm |
| Counterweight Clearance | 3.8 ft in | 1145 mm |
| Tail Swing Radius | 8.9 ft in | 2725 mm |
| Length of Track on Ground | 11 ft in | 3368 mm |