* Vermeer D33x44 **Specs**

|  |  |
| --- | --- |
| **Entry Angle** |  |
| **Fuel Tank Capacity** | 170.3 L |
| **Fuel Type** |  |
| **Ground Drive Speed** | 2.3 km/h |
| **Height** | 211 cm |
| **Hydraulic Tank Capacity** | 227 L |
| **Length** | 4.6 m |
| **Length** | 691 cm |
| **Make and Model** |  |
| **Manufacturer's Gross HP Rating** | 93 KW |
| **Max Carriage Speed** | 45.7 m/min |
| **Max Flow** | 189 LPM |
| **Max Pressure** | 83 bar |
| **Max Spindle Speed** | 234 RPM |
| **Max Spindle Torque** | 1898.2 Nm |
| **Min Bend Radius** | 33 m |
| **Min Bore Diameter** | 89 mm |
| **Pipe Diameter** | 6 cm |
| **Pullback** | 14,969 kg |
| **Rated Engine RPM** |  |
| **Rod Carrying Capacity** | 183 m |
| **Rod Loader** |  |
| **Thrust** | 89 kN |
| **Torque** | 5957 Nm |
| **Type** |  |
| **Weight** | 9,299 kg |
| **Weight** | 54 kg |
| **Width** | 208 cm |