**Delmag Foundation Rig RH 18/200**





|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| Specifications: |
| Total height | mm | 19900 |
| Drilling distance max. (center) | mm | 4000 |
| Ground clearence-mast foot | mm | 1570 |
| Inclination forward/backward | deg | 4/14 |
| Inclination left/right | deg | 9.5/9.5 |
| Crowd winch force up/down | kN | 260/150 |
| Crowd winch speed rapid/working | m/min | 25/7 |
| Stroke | mm | 12400 |

|  |
| --- |
| Base carrier: ST 25 E |
| Engine power Scania DC9 | kW | 257 |
| Track shoes | mm | 700 |
| Back pivoting radius | mm | 3230 |

|  |
| --- |
| Transport weight: |
| Transport weight with rotary head and Kelly bar K368/3-18 | kg | 60000 |

|  |
| --- |
| Transport dimensions: |
| Length | mm | 18720 |
| Width | mm | 3000 |
| Height | mm | 3400 |

  |
|  |