

**Delmag Foundation Rig RH 18/200**





|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | Specifications: | | | | Total height | mm | 19900 | | Drilling distance max. (center) | mm | 4000 | | Ground clearence-mast foot | mm | 1570 | | Inclination forward/backward | deg | 4/14 | | Inclination left/right | deg | 9.5/9.5 | | Crowd winch force up/down | kN | 260/150 | | Crowd winch speed rapid/working | m/min | 25/7 | | Stroke | mm | 12400 |  |  |  |  | | --- | --- | --- | | Base carrier: ST 25 E | | | | Engine power Scania DC9 | kW | 257 | | Track shoes | mm | 700 | | Back pivoting radius | mm | 3230 |  |  |  |  | | --- | --- | --- | | Transport weight: | | | | Transport weight with rotary head and Kelly bar K368/3-18 | kg | 60000 |  |  |  |  | | --- | --- | --- | | Transport dimensions: | | | | Length | mm | 18720 | | Width | mm | 3000 | | Height | mm | 3400 | |
|  |