**Liebherr T262 Rock Truck**



**Selected Dimensions**

|  |
| --- |
| Dimensions |
| A. Overall Length | 43.6 ft in | 13300 mm |
| B. Overall Width | 24.3 ft in | 7400 mm |
| C. Overall Height | 22 ft in | 6700 mm |
| D. Wheelbase | 20 ft in | 6100 mm |
| F. Dump Height | 19.4 ft in | 5900 mm |
| Dump |
| H. Dump Angle | 50 degrees |   |

**Specification**

|  |
| --- |
| Engine |
| Model | DDC/MTU 12V4000 |
| Gross Power | 2500 hp | 1864 kw |
| Operational |
| Fuel Capacity | 929.9 gal | 3520 L |
| Steering System Fluid Capacity | 125 gal | 473 L |
| Brake/Hoist System Fluid Capacity | 350 gal | 1325 L |
| Operating Voltage | 24 V |
| Alternator Supplied Amperage | 75 amps |
| Tire Size | 40R57 |
| Transmission |
| Max Speed | 32 mph | 51.5 km/h |
| Weights |
| Empty Weight | 345993.5 lb | 156940 kg |
| Loaded Weight | 860001.3 lb | 390090 kg |
| Dump |
| Load Capacity - Struck | 109.9 yd3 | 84 m3 |
| Load Capacity - heaped | 155.6 yd3 | 119 m3 |
| Dump Angle | 50 degrees |
| Raise Time | 21 sec |
| Lower Time | 14 sec |
| Dimensions |
| Overall Length | 43.6 ft in | 13300 mm |
| Overall Width | 24.3 ft in | 7400 mm |
| Overall Height | 22 ft in | 6700 mm |
| Wheelbase | 20 ft in | 6100 mm |
| Dump Height | 19.4 ft in | 5900 mm |