**KOMATSU pc200-6 Hydraulic Excavator**

 

**Selected Dimensions**

Boom/Stick Option

|  |  |  |
| --- | --- | --- |
| A. Shipping Length of Unit | 31.2 ft in | 9510 mm |
| C. Shipping Height of Unit | 9.8 ft in | 2985 mm |
| I. Max Cutting Height | 29.2 ft in | 8895 mm |
| J. Max Loading Height | 19.9 ft in | 6065 mm |
| K. Max Reach Along Ground | 28.6 ft in | 8720 mm |
| L. Max Vertical Wall Digging Depth | 16.3 ft in | 4965 mm |
| M. Max Digging Depth | 18.2 ft in | 5535 mm |
| Dimensions |
| B. Width to Outside of Tracks | 9.2 ft in | 2800 mm |
| D. Length of Track on Ground | 10.7 ft in | 3270 mm |
| E. Ground Clearance | 1.4 ft in | 440 mm |
| G. Height to Top of Cab | 9.5 ft in | 2905 mm |
| H. Tail Swing Radius | 9 ft in | 2750 mm |
| O. Counterweight Clearance | 3.6 ft in | 1085 mm |
| Undercarriage |
| F. Track Gauge | 7.2 ft in | 2200 mm |
| N. Shoe Size | 23.6 in | 600 mm |

**Specification**

|  |
| --- |
| Engine |
| Make | Komatsu |
| Model | S6D102E |
| Gross Power | 132.8 hp | 99 kw |
| Power Measured @ | 2200 rpm |
| Displacement | 358.8 cu in | 5.9 L |
| Number of Cylinders | 6 |
| Operational |
| Operating Weight | 42284.7 lb | 19180 kg |
| Fuel Capacity | 89.8 gal | 340 L |
| Hydrauilc System Fluid Capacity | 43.9 gal | 166 L |
| Hydraulic System Relief Valve Pressure | 5050 psi | 34818.5 kPa |
| Hydraulic Pump Flow Capacity | 108.8 gal/min | 412 L/min |
| Swing Mechanism |
| Swing Speed | 12.4 rpm |
| Undercarriage |
| Shoe Size | 23.6 in | 600 mm |
| Ground Pressure | 6.4 psi | 44.1 kPa |
| Max Travel Speed | 3.4 mph | 5.5 km/h |
| Track Gauge | 7.2 ft in | 2200 mm |
| Buckets |
| Reference Bucket Capacity | 1 yd3 | 0.8 m3 |
| Minimum Bucket Capacity | 0.65 yd3 | 0.5 m3 |
| Maximum Bucket Capacity | 1.5 yd3 | 1.2 m3 |
| Boom/Stick Option (HEX) 1 |
| Boom/Stick Option (HEX) 1 | Boom 18'8" (5700mm)/Stick 6'0" (1840mm) |
| Shipping Height of Unit | 9.8 ft in | 2985 mm |
| Shipping Length of Unit | 31.2 ft in | 9510 mm |
| Max Digging Depth | 18.2 ft in | 5535 mm |
| Max Reach Along Ground | 28.6 ft in | 8720 mm |
| Max Cutting Height | 29.2 ft in | 8895 mm |
| Max Loading Height | 19.9 ft in | 6065 mm |
| Max Vertical Wall Digging Depth | 16.3 ft in | 4965 mm |
| Boom/Stick Option (HEX) 2 |
| Boom/Stick Option (HEX) 2 | Boom 18'8" (5700mm)/Stick 7'11" (2410mm) |
| Shipping Height of Unit | 10.4 ft in | 3170 mm |
| Shipping Length of Unit | 31.1 ft in | 9485 mm |
| Max Digging Depth | 20 ft in | 6095 mm |
| Max Reach Along Ground | 30.2 ft in | 9205 mm |
| Max Cutting Height | 29.7 ft in | 9050 mm |
| Max Loading Height | 20.5 ft in | 6255 mm |
| Max Vertical Wall Digging Depth | 17.4 ft in | 5315 mm |
| Boom/Stick Option (HEX) 3 |
| Boom/Stick Option (HEX) 3 | Boom 18'8" (5700mm)/Stick 9'7" (2930mm) |
| Shipping Height of Unit | 9.7 ft in | 2970 mm |
| Shipping Length of Unit | 30.9 ft in | 9425 mm |
| Max Digging Depth | 21.7 ft in | 6620 mm |
| Max Reach Along Ground | 31.8 ft in | 9700 mm |
| Max Cutting Height | 30.5 ft in | 9305 mm |
| Max Loading Height | 21.2 ft in | 6475 mm |
| Max Vertical Wall Digging Depth | 19.6 ft in | 5980 mm |
| Boom/Stick Option (HEX) 4 |
| Boom/Stick Option (HEX) 4 | Boom 18'8" (5700mm) / Stick 13'4" (4060mm) |
| Shipping Height of Unit | 10.4 ft in | 3170 mm |
| Shipping Length of Unit | 30.9 ft in | 9425 mm |
| Max Digging Depth | 25.3 ft in | 7725 mm |
| Max Reach Along Ground | 35.7 ft in | 10880 mm |
| Max Cutting Height | 31.8 ft in | 9700 mm |
| Max Loading Height | 22.9 ft in | 6970 mm |
| Max Vertical Wall Dig Depth | 23.2 ft in | 7075 mm |
| Dimensions |
| Width to Outside of Tracks | 9.2 ft in | 2800 mm |
| Height to Top of Cab | 9.5 ft in | 2905 mm |
| Ground Clearance | 1.4 ft in | 440 mm |
| Counterweight Clearance | 3.6 ft in | 1085 mm |
| Tail Swing Radius | 9 ft in | 2750 mm |
| Length of Track on Ground | 10.7 ft in | 3270 mm |