**Kobelco K909A Specs**

**boom, stick & bucket**

|  |  |
| --- | --- |
| **Name** | **Value** |
| Bucket Width | 39.4 in |
| Bucket Capacity - Heaped | 1.05 cu yd |
| Bucket Digging Force-Standard | 27800 lbs |
| Stick Length | 113 in |
| Boom Type | 1-Piece |

**engine**

|  |  |
| --- | --- |
| **Name** | **Value** |
| Engine | 6D22C |
| Engine Manufacturer | Mitsubishi |
| Net Horsepower | 161 hp |
| Power Mode | Diesel |

**undercarriage**

|  |  |
| --- | --- |
| **Name** | **Value** |
| Track Shoe Width | 23.6 in |
| Track Length | 167 in |

**weights & dimensions**

|  |  |
| --- | --- |
| **Name** | **Value** |
| Overall Track Width--Retracted | 118 in |
| Operating Weight | 24.1 mt |