**Dresser 560B Specs**

**axles & tires**

| **Name** | **Value** |
| --- | --- |
| Tire Size | 29.5 X 29-22 (L-4) |
| Tire Size | 29.5 X 29-22(L-5) |
| Tire Size | 29.5 X 29-28(L-5) |
| Tire Size | 65/35 X 33-24(L-4) |

**bucket & loader**

| **Name** | **Value** |
| --- | --- |
| Bucket Type | Straight Edge Rock |
| Bucket Capacity - Heaped | 7.5 cu yd |
| Breakout Force | 73210 lbs |
| Bucket Width | 143.5 in |
| Bucket Width | 176 in |

**engine**

| **Name** | **Value** |
| --- | --- |
| Power Mode | Diesel |
| Engine | KT-19C |
| Engine Manufacturer | Cummins |
| Net Horsepower | 415 hp |

**operator environment**

| **Name** | **Value** |
| --- | --- |
| Operator Protection | EROPS |

**transmission**

| **Name** | **Value** |
| --- | --- |
| Number of Speeds | 3F/3R |
| Transmission Type | Powershift/TC |