
[Find a Eco Log 580B Harvester](https://www.rbauction.com/forestry-environmental?id=ci&cid=32028278347) being sold at Ritchie Bros. auctions.



**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Boom | | |
| H. Max Reach w/ Head | 37.1 ft in | 11300 mm |
| Dimensions | | |
| A. Shipping Length - non tilt | 24 ft in | 7300 mm |
| B. Overall Width | 9.8 ft in | 2990 mm |
| C. Height to Top of Cab | 15.6 ft in | 4760 mm |
| D. Wheelbase | 13 ft in | 3960 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Make | Caterpillar | |
| Model | 3126B | |
| Net Power | 225 hp | 167.8 kw |
| Displacement | 439.4 cu in | 7.2 L |
| Max Torque | 848.2 lb ft | 1150 Nm |
| Operational | | |
| Operating Weight | 39352.5 lb | 17850 kg |
| Fuel Capacity | 105.7 gal | 400 L |
| Operating Voltage | 24 V | |
| Alternator Supplied Amperage | 150 amps | |
| Max Speed | 11.2 mph | 18 km/h |
| Transmission Type | hydrostatic 6 wheel drive | |
| DRIVE SYSTEM | | |
| Number of Axels | 3 | |
| Tire Size - front | 600/55x26.5 | |
| Tire Size - rear | 710/55x34 | |
| Drive Configuration | 6 wheeldrive | |
| Boom | | |
| Max Reach w/ Head | 37.1 ft in | 11300 mm |
| Dimensions | | |
| Forward Tilt | 15 degrees | |
| Side Tilt | 25 degrees | |
| Shipping Length - non tilt | 24 ft in | 7300 mm |
| Height to Top of Cab | 15.6 ft in | 4760 mm |
| Overall Width | 9.8 ft in | 2990 mm |
| Wheelbase | 13 ft in | 3960 mm |