**Miskin D-19**

|  |  |
| --- | --- |
| Bowl capacity heaped (cu. m): | 14.53 |
| Bowl capacity struck (cu. m): | **10.02** |
| Type: | **Open** |
| Width of cut (cm): | **304.8** |
| Rear hitch for tandem: | **Std** |

**Dimensions**

|  |  |
| --- | --- |
| Length w/tongue & hitch (cm): | 817.88 |
| Width, upperstructure (cm): | **365.76** |
| Height, bowl on ground (cm): | **220.98** |

**Tractor Power**

|  |  |
| --- | --- |
| Required horsepower: | 300 |
| Max suggested horsepower: | **550** |

**Weight**

|  |  |
| --- | --- |
| Empty weight (kg): | 10886.23 |