**CATERPILLAR 657b Motor Scraper**



**Selected Dimensions**

|  |
| --- |
| Dimensions |
| A. Overall Length | 51.5 ft in | 15700 mm |
| B. Overall Width | 14.2 ft in | 4320 mm |
| C. Overall Height | 13.8 ft in | 4210 mm |

**Specification**

|  |
| --- |
| Tractor Engine |
| Make | Caterpillar |
| Gross Power | 550 hp | 410.1 kw |
| Scraper Engine |
| Make | Caterpillar |
| Gross Power | 400 hp | 298.3 kw |
| Operational |
| Tire Size | 37.5-39, 44 |
| Weights |
| Total Operating - empty | 139100 lb | 63094.7 kg |
| Bowl |
| Heaped Capactiy | 43.9 yd3 | 33.6 m3 |
| Struck Capacity | 32 yd3 | 24.5 m3 |
| Dimensions |
| Overall Length | 51.5 ft in | 15700 mm |
| Overall Width | 14.2 ft in | 4320 mm |
| Overall Height | 13.8 ft in | 4210 mm |

# Caterpillar 657B, технические характеристики.

|  |
| --- |
| Двигатель |
| Марка | **Caterpillar** |
| Мощность Мощность - измеряется в киловаттах либо лошадиных силах. Влияет на грузоподъемность. Зависит от всех параметров в двигателе внутреннего сгорания. | **410.1 кВт** |
| Двигатель |
| Марка | **Caterpillar** |
| Мощность Мощность - измеряется в киловаттах либо лошадиных силах. Влияет на грузоподъемность. Зависит от всех параметров в двигателе внутреннего сгорания. | **298.3 кВт** |
| Эксплуатационные параметры |
| Размер шин | **37.5-39, 44** |
| Масса |
| Общая эксплуатационная - пусто | **63094 кг** |
| Чаша |
| Объем ковша с шапкой | **33.6 м3** |
| Нормальный объем | **24.5 м3** |
| Размеры |
| Общая длина | **15700 мм** |
| Габаритная ширина | **4320 мм** |
| Общая высота | **4210 мм** |