
[Caterpillar CB534 Vibratory Smooth Drum Roller](https://www.rbauction.com/asphalt-concrete?id=ci&cid=32372149080)



**Selected Dimensions**

|  |  |  |
| --- | --- | --- |
| Dimensions | | |
| A. Overall Length | 16.2 ft in | 4940 mm |
| B. Overall Width | 6.1 ft in | 1850 mm |
| C. Height to Top of Cab | 7.6 ft in | 2320 mm |
| D. Wheelbase | 10.3 ft in | 3140 mm |
| E. Ground Clearance | 15 in | 380 mm |

**Specification**

|  |  |  |
| --- | --- | --- |
| Engine | | |
| Make | Caterpillar | |
| Model | 3304 | |
| Gross Power | 125 hp | 93.2 kw |
| Displacement | 427.2 cu in | 7 L |
| Operational | | |
| Operating Weight | 20099.5 lb | 9117 kg |
| Fuel Capacity | 50.2 gal | 190 L |
| Engine Oil Capacity | 5 gal | 19 L |
| Hydraulic System Fluid Capacity | 23.8 gal | 90 L |
| Max Speed | 6.8 mph | 11 km/h |
| Drum | | |
| Drum Width | 66.9 in | 1700 mm |
| Drum Diameter | 51.2 in | 1300 mm |
| Vibration Frequency 1 | 42 Hz | |
| Centrifugal Force - High | 26019 lb | 115.7 kN |
| Dimensions | | |
| Overall Length | 16.2 ft in | 4940 mm |
| Overall Width | 6.1 ft in | 1850 mm |
| Height to Top of Cab | 7.6 ft in | 2320 mm |
| Wheelbase | 10.3 ft in | 3140 mm |
| Ground Clearance | 15 in | 380 mm |