**Caterpillar 777 Rock Truck**



**Selected Dimensions**

|  |
| --- |
| Dimensions |
| A. Overall Length | 32.2 ft in | 9800 mm |
| B. Overall Width | 11.5 ft in | 3506 mm |
| C. Overall Height | 16.1 ft in | 4903 mm |
| D. Wheelbase | 15 ft in | 4572 mm |
| F. Dump Height | 30.5 ft in | 9300 mm |
| G. Dump Ground Clearance | 13.6 ft in | 4140 mm |

**Specification**

|  |
| --- |
| Engine |
| Make | Caterpillar |
| Model | D348 |
| Gross Power | 870 hp | 648.8 kw |
| Displacement | 1788 cu in | 29.3 L |
| Operational |
| Fuel Capacity | 250.2 gal | 947 L |
| Tire Size | 24x49 42 PR |
| Transmission |
| Max Speed | 36.2 mph | 58.3 km/h |
| Weights |
| Empty Weight | 124402.5 lb | 56428 kg |
| Loaded Weight | 294405.3 lb | 133540 kg |
| Dump |
| Rated Payload | 170000 lb | 77110.7 kg |
| Load Capacity - Struck | 47.5 yd3 | 36.3 m3 |
| Load Capacity - heaped | 67.1 yd3 | 51.3 m3 |
| Dimensions |
| Overall Length | 32.2 ft in | 9800 mm |
| Overall Width | 11.5 ft in | 3506 mm |
| Overall Height | 16.1 ft in | 4903 mm |
| Wheelbase | 15 ft in | 4572 mm |
| Dump Height | 30.5 ft in | 9300 mm |
| Dump Ground Clearance | 13.6 ft in | 4140 mm |